{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["实验台家具","Sheet3"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"实验台家具","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"merged":[[0,0,0,5],[2,0,7,0],[15,1,15,4],[16,0,18,0],[16,1,16,5],[17,1,17,5],[18,1,18,5]],"flags":["formulas_cached_only"]}
["家具规格参数表"]
["序号","名称","单位","规格","数量","材质说明"]
[1,"全钢台式通风柜","台","W1500*D850*H2350",1,"【柜体】采用1.2mm厚优质冷轧钢板精加工制作，金属表面经酸洗磷 ------- 化环氧树脂高温烤漆喷涂处理；                                                 【台面】采用12.7mm厚实芯理化板（耐高温、耐腐蚀、耐酸碱）；                                         【导轨】采用DTC或相同品质品牌三节式静音滑轨；                                                                                    【合页】采用3mm厚316材质不锈钢模压成型制作2片式合页；                               【拉手】采用一体成型一字型拉手或不锈钢C型拉手；                                                                【地脚】高强度可调地脚；                                                                                                                                                                        "]
[null,"1）全PP离心风机","台","3#",1,"【材质】全PP材质；                                                                                     【功率】0.3KW；                                                                                             【风量】1735-2230m3/h；                                                                             【全压】317pa；                                                                                                    【转速】1450转/分；                                                                                                                                                                          "]
[null,"2）风机软连接","套","3#",1,"【材质】5mm厚软PP材质；                                                                                                                                                                                                                         "]
[null,"3）风机减震器","只","3#",4,"【材质】阻尼弹簧减震器；                                                                                                                                                                                                                         "]
[null,"4）风机防雨帽","只","3#",1,"【材质】5mm厚PP材质；                                                                                                                                                                                                                         "]
[null,"5）通风管道","M","¢250",4,"【材质】采用UPV材质（耐腐蚀、耐酸碱、不易变形等)；                                                                                                                                                                                                                         "]
[2,"钢木靠边实验台","台","W3800*D750*H850",1,"【柜体】采用18mm厚E1级三聚氰胺板制作，所有断面经PVC防水封边处理；                                                 【台面】采用12.7mm厚实芯理化板（耐高温、耐腐蚀、耐酸碱）；                                                                                   【钢架】采用40*60*1.5mm厚方管焊接制作，金属表面经酸洗磷化环氧树脂高温烤漆喷涂处理；                                                                              【拉手】采用一字型PVC拉手或不锈钢C型拉手；                                                                                                                                                                                                                                "]
[3,"全木制吊柜","台","W3800*D450*H600",1,"【柜体】采用18mm厚E1级三聚氰胺板制作，所有断面经PVC防水封边处理；                                                                                                                          【拉手】采用一字型PVC拉手或不锈钢C型拉手；                                                                                                                                                                                                                                "]
[4,"全木制储藏架","台","W3800*D300*H440",1,"【柜体】采用18mm厚E1级三聚氰胺板制作，所有断面经PVC防水封边处理；                                                                                                                                                                                                                                                                                                                                                     "]
[5,"钢木靠边实验台","台","W2350*D750*H850",2,"【柜体】采用18mm厚E1级三聚氰胺板制作，所有断面经PVC防水封边处理；                                                 【台面】采用12.7mm厚实芯理化板（耐高温、耐腐蚀、耐酸碱）；                                                                                   【钢架】采用40*60*1.5mm厚方管焊接制作，金属表面经酸洗磷化环氧树脂高温烤漆喷涂处理；                                                                              【拉手】采用一字型PVC拉手或不锈钢C型拉手；                                                                                                                                                                                                                                "]
[6,"全木制吊柜","台","W2350*D450*H600",1,"【柜体】采用18mm厚E1级三聚氰胺板制作，所有断面经PVC防水封边处理；                                                                                                                          【拉手】采用一字型PVC拉手或不锈钢C型拉手；                                                                                                                                                                                                                                "]
[7,"全木制储藏架","台","W2350*D300*H440",1,"【柜体】采用18mm厚E1级三聚氰胺板制作，所有断面经PVC防水封边处理；                                                                                                                                                                                                                                                                                                                                                     "]
[8,"岛型插座盒及插座","套","单联单面",7,"五孔多功能10A插座；"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}